VST 3 Interfaces VST 3.7 SDK for developing VST plug-in

Public Types | Public Attributes | List of all members
BusInfo Struct Reference

BusInfo: This is the structure used with getBusInfo, informing the host about what is a specific given bus. More...

`#include <ivstcomponent.h>`

## Public Types
enum | BusFlags { kDefaultActive = 1 << 0 , kIsControlVoltage = 1 << 1 }

## Public Attributes
MediaType | mediaType
| Media type - has to be a value of MediaTypes. More...
BusDirection | direction
| input or output BusDirections More...
int32 | channelCount
| number of channels (if used then need to be recheck after IAudioProcessor::setBusArrangements is called). More...
String128 | name
| name of the bus More...
BusType | busType
| main or aux - has to be a value of BusTypes More...
uint32 | flags
| flags - a combination of BusFlags More...

## Detailed Description

BusInfo: This is the structure used with getBusInfo, informing the host about what is a specific given bus.

See also: Steinberg::Vst::IComponent::getBusInfo

## Member Enumeration Documentation

## ◆ BusFlags

enum BusFlags

Enumerator
kDefaultActive | The bus should be activated by the host per default on instantiation (activateBus call is requested). By default a bus is inactive.
kIsControlVoltage | The bus does not contain ordinary audio data, but data used for control changes at sample rate. The data is in the same format as the audio data [-1..1]. A host has to prevent unintended routing to speakers to prevent damage. Only valid for audio media type busses. [released: 3.7.0]

## Member Data Documentation

## ◆ mediaType

MediaType mediaType

Media type - has to be a value of MediaTypes.

## ◆ direction

BusDirection direction

input or output BusDirections

## ◆ channelCount

int32 channelCount

number of channels (if used then need to be recheck after IAudioProcessor::setBusArrangements is called).

For a bus of type MediaTypes::kEvent the channelCount corresponds to the number of supported MIDI channels by this bus

## ◆ name

String128 name

name of the bus

## ◆ busType

BusType busType

main or aux - has to be a value of BusTypes

## ◆ flags

uint32 flags

flags - a combination of BusFlags

Empty

Copyright © Steinberg Media Technologies GmbH. All Rights Reserved. This documentation is under this license.